\catcode`@=11
\expandafter\ifx\csname graph\endcsname\relax \alloc@4\box\chardef\insc@unt\graph\fi
\catcode`@=12
\setbox\graph=\vtop{%
  \baselineskip=0pt \lineskip=0pt \lineskiplimit=0pt
  \vbox to0pt{\hbox{%
    \special{pn 8}%
    \special{pn 20}%
    \special{pa 0 754}%
    \special{pa 0 0}%
    \special{pa 1750 0}%
    \special{pa 1750 754}%
    \special{pa 0 754}%
    \special{fp}%
    \rlap{\kern  0.875in\lower 0.320in\hbox to 0pt{\hss {USER}\hss}}%
    \rlap{\kern  0.875in\lower 0.486in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  0.875in\lower 0.350in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  0.875in\lower 0.516in\hbox to 0pt{\hss {PROGRAMS}\hss}}%
    \special{pa 0 1508}%
    \special{pa 0 754}%
    \special{pa 1750 754}%
    \special{pa 1750 1508}%
    \special{pa 0 1508}%
    \special{fp}%
    \rlap{\kern  0.875in\lower 1.074in\hbox to 0pt{\hss {LAYER 7}\hss}}%
    \rlap{\kern  0.875in\lower 1.240in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  0.875in\lower 1.104in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  0.875in\lower 1.270in\hbox to 0pt{\hss {APPLICATION}\hss}}%
    \special{pa 0 2262}%
    \special{pa 0 1508}%
    \special{pa 1750 1508}%
    \special{pa 1750 2262}%
    \special{pa 0 2262}%
    \special{fp}%
    \rlap{\kern  0.875in\lower 1.828in\hbox to 0pt{\hss {LAYER 6}\hss}}%
    \rlap{\kern  0.875in\lower 1.994in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  0.875in\lower 1.858in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  0.875in\lower 2.024in\hbox to 0pt{\hss {PRESENTATION}\hss}}%
    \special{pa 0 3016}%
    \special{pa 0 2262}%
    \special{pa 1750 2262}%
    \special{pa 1750 3016}%
    \special{pa 0 3016}%
    \special{fp}%
    \rlap{\kern  0.875in\lower 2.582in\hbox to 0pt{\hss {LAYER 5}\hss}}%
    \rlap{\kern  0.875in\lower 2.748in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  0.875in\lower 2.612in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  0.875in\lower 2.778in\hbox to 0pt{\hss {SESSION}\hss}}%
    \special{pa 0 3770}%
    \special{pa 0 3016}%
    \special{pa 1750 3016}%
    \special{pa 1750 3770}%
    \special{pa 0 3770}%
    \special{fp}%
    \rlap{\kern  0.875in\lower 3.336in\hbox to 0pt{\hss {LAYER 4}\hss}}%
    \rlap{\kern  0.875in\lower 3.502in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  0.875in\lower 3.366in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  0.875in\lower 3.532in\hbox to 0pt{\hss {TRANSPORT}\hss}}%
    \special{pa 0 4524}%
    \special{pa 0 3770}%
    \special{pa 1750 3770}%
    \special{pa 1750 4524}%
    \special{pa 0 4524}%
    \special{fp}%
    \rlap{\kern  0.875in\lower 4.090in\hbox to 0pt{\hss {LAYER 3}\hss}}%
    \rlap{\kern  0.875in\lower 4.256in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  0.875in\lower 4.120in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  0.875in\lower 4.286in\hbox to 0pt{\hss {NETWORK}\hss}}%
    \special{pa 0 5278}%
    \special{pa 0 4524}%
    \special{pa 1750 4524}%
    \special{pa 1750 5278}%
    \special{pa 0 5278}%
    \special{fp}%
    \rlap{\kern  0.875in\lower 4.844in\hbox to 0pt{\hss {LAYER 2}\hss}}%
    \rlap{\kern  0.875in\lower 5.010in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  0.875in\lower 4.874in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  0.875in\lower 5.040in\hbox to 0pt{\hss {DATA LINK}\hss}}%
    \special{pa 0 6032}%
    \special{pa 0 5278}%
    \special{pa 1750 5278}%
    \special{pa 1750 6032}%
    \special{pa 0 6032}%
    \special{fp}%
    \rlap{\kern  0.875in\lower 5.598in\hbox to 0pt{\hss {LAYER 1}\hss}}%
    \rlap{\kern  0.875in\lower 5.764in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  0.875in\lower 5.628in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  0.875in\lower 5.794in\hbox to 0pt{\hss {PHYSICAL}\hss}}%
    \rlap{\kern  5.250in\lower 0.320in\hbox to 0pt{\hss \hbox to 6.0in{MMFS/EIA 1393A\hfil}\hss}}%
    \rlap{\kern  5.250in\lower 0.486in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  5.250in\lower 0.350in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  5.250in\lower 0.516in\hbox to 0pt{\hss \hbox to 6.0in{(OBSOLETED IN MAP 3.0)\hfil}\hss}}%
    \rlap{\kern  5.250in\lower 1.074in\hbox to 0pt{\hss \hbox to 6.0in{[DRAFT ISO 8571/1-4] FILE TRANSFER, ACCESS AND\hfil}\hss}}%
    \rlap{\kern  5.250in\lower 1.240in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  5.250in\lower 1.104in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  5.250in\lower 1.270in\hbox to 0pt{\hss \hbox to 6.0in{\hphantom{[DRAFT ISO 8571/1-4]} MANAGEMENT SERVICE (FTAM)\hfil}\hss}}%
    \rlap{\kern  5.250in\lower 1.926in\hbox to 0pt{\hss \hbox to 6.0in{NONE AT THIS TIME\hfil}\hss}}%
    \rlap{\kern  5.250in\lower 2.680in\hbox to 0pt{\hss \hbox to 6.0in{[ISO 8326/7] KERNEL SUBSET OF SESSION SERVICE\hfil}\hss}}%
    \rlap{\kern  5.250in\lower 3.434in\hbox to 0pt{\hss \hbox to 6.0in{[ISO 8072/3] TRANSPORT SERVICE - CLASS 4 (TP4)\hfil}\hss}}%
    \rlap{\kern  5.250in\lower 4.188in\hbox to 0pt{\hss \hbox to 6.0in{[ISO 8473] CONNECTIONLESS NETWORK SERVICE\hfil}\hss}}%
    \rlap{\kern  5.250in\lower 4.942in\hbox to 0pt{\hss \hbox to 6.0in{[ISO 8802/2] IEEE 802.2 LOGICAL LINK CONTROL\hfil}\hss}}%
    \rlap{\kern  5.250in\lower 5.598in\hbox to 0pt{\hss \hbox to 6.0in{[ISO 8802/4] IEEE 802.4 TOKEN BUS (MAP 2.1)\hfil}\hss}}%
    \rlap{\kern  5.250in\lower 5.764in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  5.250in\lower 5.628in\hbox to 0pt{\hss  \hss}}%
    \rlap{\kern  5.250in\lower 5.794in\hbox to 0pt{\hss \hbox to 6.0in{[ISO 8802/3] IEEE 802.3 CSMA/CD (TOP 1.0)\hfil}\hss}}%
    \special{pn 1}%
    \special{pa 7500 4901}%
    \special{pa 7501 4901}%
    \special{dt  0.050}%
    \kern  7.502in
  }\vss}%
  \kern  6.033in
}
